* Lưu ý: toàn bộ module cần giao diện, chạy qua remote desktop 10.149.3.125, đã cài đặt sẵn Xshell (Administrator/root@123)
* Structure

IP: 10.149.3.x/25

GW: 10.149.3.1

|  |  |  |  |
| --- | --- | --- | --- |
| **Server Name** | **IP address** | **App server name** | **Notes** |
| slu-base-13 | 10.149.3.116/25 | SFTP server 1 | Pull file CDR từ UPM về |
| slu-base-14 | 10.149.3.117/25 | SFTP server 2 | RC & Aggregate & eDatasync |
| slu-base-15 | 10.149.3.118/25 | Standby server 1 |  |
| slu-base-16 | 10.149.3.119/25 | Reformat server 1 |  |
| slu-base-17 | 10.149.3.120/25 | Reformat server 2 |  |
| **slu-base-18** | **10.149.3.121/25** | **Re-rate server 1** |  |
| **slu-base-19** | **10.149.3.122/25** | **Re-rate server 2** |  |
| slu-base-20 | 10.149.3.123/25 | RC rating server | ORP transformation + pull/push CDR |
| slu-base-21 | 10.149.3.124/25 | Aggregate rating server | ORP transformation + pull/push CDR |
| slu-base-22 | 10.149.3.125/25 | Standby server 2 | Cài Windows Server |
| rac-node-1 | 10.149.3.113 | Database RAC node1 |  |
| rac-node-1 | 10.149.3.113 | Database RAC node1 |  |
| **VNP** |  |  |  |
| VNP ORP CDR 01 | 10.149.33.214 |  | ssh: elcom/elcom@123456 |
| VNP ORP CDR 02 | 10.149.33.215 |  | ssh: elcom/elcom@123456 |

